
// File generated by darts version X-2025.06#84ea4f0b1c#250602, Thu Mar 26 14:37:59 2026
// Copyright 2014-2025 Synopsys, Inc. All rights reserved.
// C:\Synopsys\ASIP Programmer\X-2025.06\win64\bin\WINbin\darts.exe -IC:/Users/phangl/OneDrive - MED-EL/Desktop/LPDSP32_Modell/lib -d -IC:/Users/phangl/OneDrive - MED-EL/Desktop/LPDSP32_Modell/lib/runtime/include -DBLOCK_LEN=1 -DMAX_FIR_COEFFS=45 -D__tct_patch__=0 +Mhex +Ihex -g Release/signal_path.o lpdsp32

// Release: ipp X-2025.06
.data_segment_name
.bss local 4 _ZL7counter DMA 4

.data_segment_name
.bss local 4 _ZL2mu DMA 4

.data_segment_name
.data local 4 _ZL4leak DMA
	0x1d
	0xac
	0xff
	0x7f

.data_segment_name
.bss local 4 _ZZ16calculate_outputP4FILEP16SingleSignalPathS2_PU17chess_storage_DMBVsS4_S4_E11c_sensor_32 DMA 4

.data_segment_name
.bss local 4 _ZZ16calculate_outputP4FILEP16SingleSignalPathS2_PU17chess_storage_DMBVsS4_S4_E13acc_sensor_32 DMA 4

.data_segment_name
.bss local 4 _ZZ16calculate_outputP4FILEP16SingleSignalPathS2_PU17chess_storage_DMBVsS4_S4_E12c_sensor_pre DMA 4

.data_segment_name
.bss local 4 _ZZ16calculate_outputP4FILEP16SingleSignalPathS2_PU17chess_storage_DMBVsS4_S4_E14acc_sensor_pre DMA 4

.data_segment_name
.bss local 4 _ZZ16calculate_outputP4FILEP16SingleSignalPathS2_PU17chess_storage_DMBVsS4_S4_E18filter_accumulator DMB 4

.data_segment_name
.bss local 4 _ZZ16calculate_outputP4FILEP16SingleSignalPathS2_PU17chess_storage_DMBVsS4_S4_E9output_32 DMB 4

.undef local data _Z16calculate_outputP4FILEP16SingleSignalPathS2_PU17chess_storage_DMBVsS4_S4___end

.undef local data _ZL2mu

.undef local data _ZZ16calculate_outputP4FILEP16SingleSignalPathS2_PU17chess_storage_DMBVsS4_S4_E11c_sensor_32

.undef local data _ZZ16calculate_outputP4FILEP16SingleSignalPathS2_PU17chess_storage_DMBVsS4_S4_E13acc_sensor_32

.undef local data _ZZ16calculate_outputP4FILEP16SingleSignalPathS2_PU17chess_storage_DMBVsS4_S4_E12c_sensor_pre

.undef local data _ZZ16calculate_outputP4FILEP16SingleSignalPathS2_PU17chess_storage_DMBVsS4_S4_E14acc_sensor_pre

.undef local data _ZZ16calculate_outputP4FILEP16SingleSignalPathS2_PU17chess_storage_DMBVsS4_S4_E18filter_accumulator

.undef local data _ZZ16calculate_outputP4FILEP16SingleSignalPathS2_PU17chess_storage_DMBVsS4_S4_E9output_32

.undef local data _ZL2mu

.data_segment_name
.bss global 4 sample_line DMB 180

.data_segment_name
.bss global 8 coefficient_line DMA 180

.data_segment_name
.bss global 4 pointer_sample_line DMB 12

.data_segment_name
.bss global 4 pointer_coefficient_line DMA 12

.undef global data stdin

.undef global data stdout

.undef global data _Z16calculate_outputP4FILEP16SingleSignalPathS2_PU17chess_storage_DMBVsS4_S4_

.text_segment_name
.text global 2 _Z17initialize_bufferP9BufferPtrPiii
.src_ref 0 "signal_path.c" 137 first
.src_ref 0 "signal_path.c" 138 10
.src_ref 0 "signal_path.c" 143 24
	/* 0x000000 0x39020 */    c0 = 4
.src_ref 0 "signal_path.c" 138 10 first
.src_ref 0 "signal_path.c" 142 4 first
	/* 0x000001 0x59014 */    cmp(ra1,0x0); [a0+c0] = ra1
	/* 0x000002 0x00049 */    /* MW */
.src_ref 0 "signal_path.c" 140 10 first
.src_ref 0 "signal_path.c" 142 4
	/* 0x000003 0x42036 */    if (np) jpsdb 0x6; a0[0x4] = a1
	/* 0x000004 0x840e1 */    /* MW */
.src_ref 0 "signal_path.c" 139 10 first
	/* 0x000005 0x84061 */    a0[0x0] = a1
.src_ref 0 "signal_path.c" 142 4 first
	/* 0x000006 0x62000 */    lp [ra1] 0x1
	/* 0x000007 0x00015 */    /* MW */
	/* 0x000008 0x00000 */    nop
	/* 0x000009 0x00000 */    nop
.src_ref 0 "signal_path.c" 143 24 first
	/* 0x00000a 0x8087a */    [a1+c0] = zero
.src_ref 0 "signal_path.c" 145 14 first
	/* 0x00000b 0x301a8 */    cmp(ra1,rb0)
.src_ref 0 "signal_path.c" 145 4
.src_ref 0 "signal_path.c" 145 14
	/* 0x00000c 0x42011 */    if (s) jps 0x2; ra0 = zero
	/* 0x00000d 0x18e88 */    /* MW */
.src_ref 0 "signal_path.c" 145 4
	/* 0x00000e 0x5c006 */    ra0 = 1; ret
	/* 0x00000f 0x3a140 */    /* MW */
.label _Z17initialize_bufferP9BufferPtrPiii__end last
.src_ref 0 "signal_path.c" 145 4
	/* 0x000010 0x40000 */    nop; ret
	/* 0x000011 0x3a140 */    /* MW */

.text_segment_name
.text global 2 _Z21initialize_buffer_dmbPU17chess_storage_DMB12BufferPtrDMBPU17chess_storage_DMBiii
.src_ref 0 "signal_path.c" 154 first
.src_ref 0 "signal_path.c" 155 10
.src_ref 0 "signal_path.c" 160 24
	/* 0x000000 0x39020 */    c0 = 4
.src_ref 0 "signal_path.c" 155 10 first
.src_ref 0 "signal_path.c" 159 4 first
	/* 0x000001 0x59014 */    cmp(ra1,0x0); [a4+c0] = ra1
	/* 0x000002 0x02049 */    /* MW */
.src_ref 0 "signal_path.c" 157 10 first
.src_ref 0 "signal_path.c" 159 4
	/* 0x000003 0x42036 */    if (np) jpsdb 0x6; a4[0x4] = a5
	/* 0x000004 0x860e5 */    /* MW */
.src_ref 0 "signal_path.c" 156 10 first
	/* 0x000005 0x86065 */    a4[0x0] = a5
.src_ref 0 "signal_path.c" 159 4 first
	/* 0x000006 0x62000 */    lp [ra1] 0x1
	/* 0x000007 0x00015 */    /* MW */
	/* 0x000008 0x00000 */    nop
	/* 0x000009 0x00000 */    nop
.src_ref 0 "signal_path.c" 160 24 first
	/* 0x00000a 0x8287a */    [a5+c0] = zero
.src_ref 0 "signal_path.c" 162 14 first
	/* 0x00000b 0x301a8 */    cmp(ra1,rb0)
.src_ref 0 "signal_path.c" 162 4
.src_ref 0 "signal_path.c" 162 14
	/* 0x00000c 0x42011 */    if (s) jps 0x2; ra0 = zero
	/* 0x00000d 0x18e88 */    /* MW */
.src_ref 0 "signal_path.c" 162 4
	/* 0x00000e 0x5c006 */    ra0 = 1; ret
	/* 0x00000f 0x3a140 */    /* MW */
.label _Z21initialize_buffer_dmbPU17chess_storage_DMB12BufferPtrDMBPU17chess_storage_DMBiii__end last
.src_ref 0 "signal_path.c" 162 4
	/* 0x000010 0x40000 */    nop; ret
	/* 0x000011 0x3a140 */    /* MW */

.text_segment_name
.text global 2 _Z12write_bufferP9BufferPtri
.src_ref 0 "signal_path.c" 172 11
.src_ref 0 "signal_path.c" 172 11 first
.src_ref 0 "signal_path.c" 173 26
.src_ref 0 "signal_path.c" 173 67
.src_ref 0 "signal_path.c" 174 first
	/* 0x000000 0x5c810 */    c0 = 4; a0 = a0 + 0x8
	/* 0x000001 0x20040 */    /* MW */
.src_ref 0 "signal_path.c" 172 11 first
	/* 0x000002 0x80221 */    a1 = [a0-c0]
.src_ref 0 "signal_path.c" 173 67 first
	/* 0x000003 0x8022c */    lb0 = [a0-c0]
.src_ref 0 "signal_path.c" 172 4 first
	/* 0x000004 0x84848 */    a1[0x0] = ra0
	/* 0x000005 0x00000 */    nop
.src_ref 0 "signal_path.c" 173 86 first
	/* 0x000006 0x84008 */    ra0 = a0[0x0]
.src_ref 0 "signal_path.c" 173 86
	/* 0x000007 0x230a4 */    ra0 = lsl(ra0,0x2)
.src_ref 0 "signal_path.c" 173 26
	/* 0x000008 0x9822e */    lsz0 = ra0
	/* 0x000009 0x00000 */    nop
.src_ref 0 "signal_path.c" 173 26
.src_ref 0 "signal_path.c" 174 first
	/* 0x00000a 0x460a4 */    retdb; a1 = a1+%0c0
	/* 0x00000b 0x1cc01 */    /* MW */
.src_ref 0 "signal_path.c" 173 10 first
	/* 0x00000c 0x84161 */    a0[0x8] = a1
.label _Z12write_bufferP9BufferPtri__end
	/* 0x00000d 0x00000 */    nop

.text_segment_name
.text global 2 _Z16write_buffer_dmbPU17chess_storage_DMB12BufferPtrDMBi
.src_ref 0 "signal_path.c" 178 11
.src_ref 0 "signal_path.c" 178 11 first
.src_ref 0 "signal_path.c" 179 26
.src_ref 0 "signal_path.c" 179 67
.src_ref 0 "signal_path.c" 180 first
	/* 0x000000 0x5c810 */    c0 = 4; a4 = a4 + 0x8
	/* 0x000001 0x22044 */    /* MW */
.src_ref 0 "signal_path.c" 178 11 first
	/* 0x000002 0x82220 */    a0 = [a4-c0]
.src_ref 0 "signal_path.c" 179 67 first
	/* 0x000003 0x8222c */    lb0 = [a4-c0]
.src_ref 0 "signal_path.c" 178 4 first
	/* 0x000004 0x84048 */    a0[0x0] = ra0
	/* 0x000005 0x00000 */    nop
.src_ref 0 "signal_path.c" 179 86 first
	/* 0x000006 0x86008 */    ra0 = a4[0x0]
.src_ref 0 "signal_path.c" 179 86
	/* 0x000007 0x230a4 */    ra0 = lsl(ra0,0x2)
.src_ref 0 "signal_path.c" 179 26
	/* 0x000008 0x9822e */    lsz0 = ra0
	/* 0x000009 0x00000 */    nop
.src_ref 0 "signal_path.c" 179 26
.src_ref 0 "signal_path.c" 180 first
	/* 0x00000a 0x460a4 */    retdb; a0 = a0+%0c0
	/* 0x00000b 0x1c400 */    /* MW */
.src_ref 0 "signal_path.c" 179 10 first
	/* 0x00000c 0x86160 */    a4[0x8] = a0
.label _Z16write_buffer_dmbPU17chess_storage_DMB12BufferPtrDMBi__end
	/* 0x00000d 0x00000 */    nop

.data_segment_name
.rodata.constmem global 8 _ro_data_DM_8___Z20scale_preemph_filterP16SingleSignalPathdddddi__2 DM
.label _ro_lbl_DM_8___Z20scale_preemph_filterP16SingleSignalPathdddddi_0_0
	0x0
	0x0
	0x0
	0x0
	0x0
	0x0
	0xf0
	0x3f
.label _ro_lbl_DM_8___Z20scale_preemph_filterP16SingleSignalPathdddddi_8_1
	0x0
	0x0
	0x0
	0x0
	0x0
	0x0
	0x0
	0x40

.text_segment_name
.text global 2 _Z20scale_preemph_filterP16SingleSignalPathdddddi
.src_ref 0 "signal_path.c" 183 first
.src_ref 0 "signal_path.c" 183 5
	/* 0x000000 0xabfa0 */    sp+= -0x30
	/* 0x000001 0x90259 */    sp[0x10] = ahl1
	/* 0x000002 0x880f6 */    sp[0x4] = lr
	/* 0x000003 0x88048 */    sp[0x0] = ra0
	/* 0x000004 0x9035b */    sp[0x18] = bhl1
	/* 0x000005 0x9045a */    sp[0x20] = bhl0
	/* 0x000006 0x90558 */    sp[0x28] = ahl0
	/* 0x000007 0x88160 */    sp[0x8] = a0
.src_ref 0 "signal_path.c" 185 11 first
	/* 0x000008 0x66000 */    calldb _Z10float64_eqyy
	/* 0x000009 0x00008 */    /* MW */
.src_ref 0 "signal_path.c" 185 11
	/* 0x00000a 0x6e000 */    axl1 = [_ro_lbl_DM_8___Z20scale_preemph_filterP16SingleSignalPathdddddi_0_0]
	/* 0x00000b 0x00011 */    /* MW */
.src_ref 0 "signal_path.c" 185 11
.src_ref 0 "signal_path.c" 186 14
.src_ref 0 "signal_path.c" 189 14
	/* 0x00000c 0x59010 */    cmp(ra0,0x0); a1 = sp[0x8]
	/* 0x00000d 0x08121 */    /* MW */
.src_ref 0 "signal_path.c" 185 11
.src_ref 0 "signal_path.c" 185 17
	/* 0x00000e 0xbc298 */    if (z) jpsdb 0x29
.src_ref 0 "signal_path.c" 186 14 first
	/* 0x00000f 0xa0840 */    a0 = a1 + 0x8
	/* 0x000010 0x40000 */    nop; sp[0xc] = a0
	/* 0x000011 0x081e0 */    /* MW */
.src_ref 0 "signal_path.c" 185 23 first
	/* 0x000012 0x66000 */    calldb _Z10float64_eqyy
	/* 0x000013 0x00008 */    /* MW */
.src_ref 0 "signal_path.c" 185 23
.src_ref 0 "signal_path.c" 185 23
	/* 0x000014 0x5c000 */    ax1 = 0; axl0 = sp[0x10]
	/* 0x000015 0x90210 */    /* MW */
.src_ref 0 "signal_path.c" 185 23
.src_ref 0 "signal_path.c" 190 14
	/* 0x000016 0x59010 */    cmp(ra0,0x0); a0 = sp[0xc]
	/* 0x000017 0x081a0 */    /* MW */
.src_ref 0 "signal_path.c" 185 23
.src_ref 0 "signal_path.c" 185 29
.src_ref 0 "signal_path.c" 186 14
.src_ref 0 "signal_path.c" 189 14
	/* 0x000018 0x420f0 */    if (z) jps 0x1e; a1 = sp[0x8]
	/* 0x000019 0x08121 */    /* MW */
	/* 0x00001a 0x40000 */    nop; sp[0xc] = a0
	/* 0x00001b 0x081e0 */    /* MW */
.src_ref 0 "signal_path.c" 185 35
	/* 0x00001c 0x66000 */    calldb _Z10float64_eqyy
	/* 0x00001d 0x00008 */    /* MW */
.src_ref 0 "signal_path.c" 185 35
.src_ref 0 "signal_path.c" 185 35
	/* 0x00001e 0x5c000 */    ax1 = 0; axl0 = sp[0x20]
	/* 0x00001f 0x90410 */    /* MW */
.src_ref 0 "signal_path.c" 185 35
.src_ref 0 "signal_path.c" 190 14
	/* 0x000020 0x59010 */    cmp(ra0,0x0); a0 = sp[0xc]
	/* 0x000021 0x081a0 */    /* MW */
.src_ref 0 "signal_path.c" 185 35
.src_ref 0 "signal_path.c" 185 41
.src_ref 0 "signal_path.c" 186 14
.src_ref 0 "signal_path.c" 189 14
	/* 0x000022 0x420a0 */    if (z) jps 0x14; a1 = sp[0x8]
	/* 0x000023 0x08121 */    /* MW */
	/* 0x000024 0x40000 */    nop; sp[0xc] = a0
	/* 0x000025 0x081e0 */    /* MW */
.src_ref 0 "signal_path.c" 185 47
	/* 0x000026 0x66000 */    calldb _Z10float64_eqyy
	/* 0x000027 0x00008 */    /* MW */
.src_ref 0 "signal_path.c" 185 47
.src_ref 0 "signal_path.c" 185 47
	/* 0x000028 0x5c000 */    ax1 = 0; axl0 = sp[0x18]
	/* 0x000029 0x90310 */    /* MW */
.src_ref 0 "signal_path.c" 185 47
.src_ref 0 "signal_path.c" 190 14
	/* 0x00002a 0x59010 */    cmp(ra0,0x0); a0 = sp[0xc]
	/* 0x00002b 0x081a0 */    /* MW */
.src_ref 0 "signal_path.c" 185 47
.src_ref 0 "signal_path.c" 185 53
.src_ref 0 "signal_path.c" 186 14
.src_ref 0 "signal_path.c" 189 14
	/* 0x00002c 0x42050 */    if (z) jps 0xa; a1 = sp[0x8]
	/* 0x00002d 0x08121 */    /* MW */
	/* 0x00002e 0x40000 */    nop; sp[0xc] = a0
	/* 0x00002f 0x081e0 */    /* MW */
.src_ref 0 "signal_path.c" 185 59
	/* 0x000030 0x66000 */    calldb _Z10float64_eqyy
	/* 0x000031 0x00008 */    /* MW */
.src_ref 0 "signal_path.c" 185 59
.src_ref 0 "signal_path.c" 185 59
	/* 0x000032 0x5c000 */    ax1 = 0; axl0 = sp[0x30]
	/* 0x000033 0x90610 */    /* MW */
.src_ref 0 "signal_path.c" 185 59
.src_ref 0 "signal_path.c" 186 14
.src_ref 0 "signal_path.c" 189 14
	/* 0x000034 0x59010 */    cmp(ra0,0x0); a1 = sp[0x8]
	/* 0x000035 0x08121 */    /* MW */
.src_ref 0 "signal_path.c" 185 4
.src_ref 0 "signal_path.c" 185 59
.src_ref 0 "signal_path.c" 190 14
	/* 0x000036 0x42248 */    if (nz) jps 0x49; a0 = sp[0xc]
	/* 0x000037 0x881a0 */    /* MW */
.src_ref 0 "signal_path.c" 190 14
.src_ref 0 "signal_path.c" 191 25
	/* 0x000038 0x88008 */    ra0 = sp[0x0]
.src_ref 0 "signal_path.c" 189 14
.src_ref 0 "signal_path.c" 190 14
	/* 0x000039 0x5c007 */    rb0 = 1; a0 = a0 + 0x18
	/* 0x00003a 0x200c0 */    /* MW */
.src_ref 0 "signal_path.c" 190 14 first
	/* 0x00003b 0x84048 */    a0[0x0] = ra0
.src_ref 0 "signal_path.c" 193 14
	/* 0x00003c 0xa04a0 */    a0 = a0 - 0x14
	/* 0x00003d 0x88060 */    sp[0x0] = a0
.src_ref 0 "signal_path.c" 189 14 first
	/* 0x00003e 0x8494a */    a1[0x8] = rb0
.src_ref 0 "signal_path.c" 191 25 first
	/* 0x00003f 0x66000 */    call _Z16int32_to_float64i
	/* 0x000040 0x00000 */    /* MW */
.src_ref 0 "signal_path.c" 191 20
	/* 0x000041 0x2a002 */    bx0 = ax0 + 0x0
.src_ref 0 "signal_path.c" 191 20
	/* 0x000042 0x66000 */    calldb ff_pow
	/* 0x000043 0x00008 */    /* MW */
.src_ref 0 "signal_path.c" 191 20
	/* 0x000044 0x6e000 */    axl1 = [(_ro_lbl_DM_8___Z20scale_preemph_filterP16SingleSignalPathdddddi_8_1 + 0)]
	/* 0x000045 0x00411 */    /* MW */
.src_ref 0 "signal_path.c" 191 39
	/* 0x000046 0x55000 */    ax1 = ax0 + 0x0; nop
	/* 0x000047 0xb8000 */    /* MW */
.src_ref 0 "signal_path.c" 191 39
	/* 0x000048 0x66000 */    calldb _Z11float64_subyy
	/* 0x000049 0x00008 */    /* MW */
.src_ref 0 "signal_path.c" 191 39
	/* 0x00004a 0x6e000 */    bxl0 = [_ro_lbl_DM_8___Z20scale_preemph_filterP16SingleSignalPathdddddi_0_0]
	/* 0x00004b 0x00012 */    /* MW */
.src_ref 0 "signal_path.c" 191 39
	/* 0x00004c 0x66000 */    call _Z30float64_to_int32_round_to_zeroy
	/* 0x00004d 0x00000 */    /* MW */
.src_ref 0 "signal_path.c" 193 34 first
	/* 0x00004e 0x66000 */    call _Z16int32_to_float64i
	/* 0x00004f 0x00000 */    /* MW */
.src_ref 0 "signal_path.c" 193 34
.src_ref 0 "signal_path.c" 193 34
	/* 0x000050 0x55001 */    bx0 = ax0 + 0x0; axl1 = sp[0x28]
	/* 0x000051 0x10511 */    /* MW */
	/* 0x000052 0x40000 */    nop; sp[0x8] = bhl0
	/* 0x000053 0x1015a */    /* MW */
.src_ref 0 "signal_path.c" 193 34
	/* 0x000054 0x66000 */    call _Z11float64_mulyy
	/* 0x000055 0x00000 */    /* MW */
.src_ref 0 "signal_path.c" 193 29
	/* 0x000056 0x66000 */    call _Z30float64_to_int32_round_to_zeroy
	/* 0x000057 0x00000 */    /* MW */
.src_ref 0 "signal_path.c" 193 25
	/* 0x000058 0x88020 */    a0 = sp[0x0]
.src_ref 0 "signal_path.c" 193 25
.src_ref 0 "signal_path.c" 194 34
	/* 0x000059 0x5c810 */    c0 = 4; bxl0 = sp[0x8]
	/* 0x00005a 0x10112 */    /* MW */
.src_ref 0 "signal_path.c" 193 25
	/* 0x00005b 0x80048 */    [a0+c0] = ra0
	/* 0x00005c 0x88060 */    sp[0x0] = a0
.src_ref 0 "signal_path.c" 194 34 first
	/* 0x00005d 0x66000 */    calldb _Z11float64_mulyy
	/* 0x00005e 0x00008 */    /* MW */
.src_ref 0 "signal_path.c" 194 34
	/* 0x00005f 0x90211 */    axl1 = sp[0x10]
.src_ref 0 "signal_path.c" 194 29
	/* 0x000060 0x66000 */    call _Z30float64_to_int32_round_to_zeroy
	/* 0x000061 0x00000 */    /* MW */
.src_ref 0 "signal_path.c" 194 25
	/* 0x000062 0x88020 */    a0 = sp[0x0]
.src_ref 0 "signal_path.c" 194 25
.src_ref 0 "signal_path.c" 195 34
	/* 0x000063 0x5c810 */    c0 = 4; bxl0 = sp[0x8]
	/* 0x000064 0x10112 */    /* MW */
.src_ref 0 "signal_path.c" 194 25
	/* 0x000065 0x80048 */    [a0+c0] = ra0
	/* 0x000066 0x88060 */    sp[0x0] = a0
.src_ref 0 "signal_path.c" 195 34 first
	/* 0x000067 0x66000 */    calldb _Z11float64_mulyy
	/* 0x000068 0x00008 */    /* MW */
.src_ref 0 "signal_path.c" 195 34
	/* 0x000069 0x90411 */    axl1 = sp[0x20]
.src_ref 0 "signal_path.c" 195 29
	/* 0x00006a 0x66000 */    call _Z30float64_to_int32_round_to_zeroy
	/* 0x00006b 0x00000 */    /* MW */
.src_ref 0 "signal_path.c" 195 25
	/* 0x00006c 0x88020 */    a0 = sp[0x0]
.src_ref 0 "signal_path.c" 195 25
.src_ref 0 "signal_path.c" 196 34
	/* 0x00006d 0x5c810 */    c0 = 4; bxl0 = sp[0x8]
	/* 0x00006e 0x10112 */    /* MW */
.src_ref 0 "signal_path.c" 195 25
	/* 0x00006f 0x80048 */    [a0+c0] = ra0
	/* 0x000070 0x88260 */    sp[0x10] = a0
.src_ref 0 "signal_path.c" 196 34 first
	/* 0x000071 0x66000 */    calldb _Z11float64_mulyy
	/* 0x000072 0x00008 */    /* MW */
.src_ref 0 "signal_path.c" 196 34
	/* 0x000073 0x90311 */    axl1 = sp[0x18]
.src_ref 0 "signal_path.c" 196 29
	/* 0x000074 0x66000 */    call _Z30float64_to_int32_round_to_zeroy
	/* 0x000075 0x00000 */    /* MW */
.src_ref 0 "signal_path.c" 196 25
	/* 0x000076 0x88020 */    a0 = sp[0x0]
.src_ref 0 "signal_path.c" 197 34
	/* 0x000077 0x90112 */    bxl0 = sp[0x8]
.src_ref 0 "signal_path.c" 196 25
	/* 0x000078 0x840c8 */    a0[0x4] = ra0
.src_ref 0 "signal_path.c" 197 34 first
	/* 0x000079 0x66000 */    calldb _Z11float64_mulyy
	/* 0x00007a 0x00008 */    /* MW */
.src_ref 0 "signal_path.c" 197 34
	/* 0x00007b 0x90611 */    axl1 = sp[0x30]
.src_ref 0 "signal_path.c" 197 29
	/* 0x00007c 0x66000 */    call _Z30float64_to_int32_round_to_zeroy
	/* 0x00007d 0x00000 */    /* MW */
.src_ref 0 "signal_path.c" 197 25
	/* 0x00007e 0x88220 */    a0 = sp[0x10]
	/* 0x00007f 0xbc02f */    jpsdb 0x2
.src_ref 0 "signal_path.c" 197 25
	/* 0x000080 0x840c8 */    a0[0x4] = ra0
.src_ref 0 "signal_path.c" 186 14 first
	/* 0x000081 0x8497a */    a1[0x8] = zero
	/* 0x000082 0x00000 */    nop
.src_ref 0 "signal_path.c" 199
	/* 0x000083 0x880b6 */    lr = sp[0x4]
.label _Z20scale_preemph_filterP16SingleSignalPathdddddi__end last
.src_ref 0 "signal_path.c" 199 first
.src_ref 0 "signal_path.c" 199 first
	/* 0x000084 0x460a0 */    ret; sp+= 0x30
	/* 0x000085 0x28060 */    /* MW */

.undef global text ff_pow

.undef global text _Z10float64_eqyy

.undef global text _Z16int32_to_float64i

.undef global text _Z11float64_subyy

.undef global text _Z30float64_to_int32_round_to_zeroy

.undef global text _Z11float64_mulyy

.text_segment_name
.text global 2 _Z9set_delayP16SingleSignalPathi
.src_ref 0 "signal_path.c" 202 first
.src_ref 0 "signal_path.c" 203 36 first
	/* 0x000000 0x40000 */    nop; a0 = a0 + 0x74
	/* 0x000001 0x203a0 */    /* MW */
.src_ref 0 "signal_path.c" 203 11 first
	/* 0x000002 0x64000 */    jpdb _Z17initialize_bufferP9BufferPtrPiii
	/* 0x000003 0x0000f */    /* MW */
.label _Z9set_delayP16SingleSignalPathi__end last
.src_ref 0 "signal_path.c" 203 11
.src_ref 0 "signal_path.c" 203 58
	/* 0x000004 0x5c043 */    rb0 = 16; a1 = a0 - 0x40
	/* 0x000005 0x20601 */    /* MW */

.undef global text _Z17initialize_bufferP9BufferPtrPiii

.data_segment_name
.rodata.constmem global 8 _ro_data_DM_8___Z10set_weightP16SingleSignalPathdi__2 DM
.label _ro_lbl_DM_8___Z10set_weightP16SingleSignalPathdi_0_0
	0x0
	0x0
	0x0
	0x0
	0x0
	0x0
	0xf0
	0x3f
.label _ro_lbl_DM_8___Z10set_weightP16SingleSignalPathdi_8_1
	0x0
	0x0
	0x0
	0x0
	0x0
	0x0
	0x0
	0x40

.text_segment_name
.text global 2 _Z10set_weightP16SingleSignalPathdi
.src_ref 0 "signal_path.c" 207 first
.src_ref 0 "signal_path.c" 207 5
	/* 0x000000 0xabfd0 */    sp+= -0x18
	/* 0x000001 0x88076 */    sp[0x0] = lr
	/* 0x000002 0x880c8 */    sp[0x4] = ra0
	/* 0x000003 0x90258 */    sp[0x10] = ahl0
	/* 0x000004 0x88160 */    sp[0x8] = a0
.src_ref 0 "signal_path.c" 209 15 first
	/* 0x000005 0x66000 */    calldb _Z10float64_eqyy
	/* 0x000006 0x00008 */    /* MW */
.src_ref 0 "signal_path.c" 209 15
	/* 0x000007 0x6e000 */    axl1 = [_ro_lbl_DM_8___Z10set_weightP16SingleSignalPathdi_0_0]
	/* 0x000008 0x00011 */    /* MW */
.src_ref 0 "signal_path.c" 210 14
	/* 0x000009 0x88120 */    a0 = sp[0x8]
.src_ref 0 "signal_path.c" 209 15
	/* 0x00000a 0x32020 */    cmp(ra0,0x0)
.src_ref 0 "signal_path.c" 210 14 first
	/* 0x00000b 0x76000 */    a0 = a0 + 0x84
	/* 0x00000c 0x00420 */    /* MW */
.src_ref 0 "signal_path.c" 209 4 first
.src_ref 0 "signal_path.c" 209 15 first
	/* 0x00000d 0x42110 */    if (nz) jps 0x22; sp[0x8] = a0
	/* 0x00000e 0x88160 */    /* MW */
.src_ref 0 "signal_path.c" 214 14
	/* 0x00000f 0x3800c */    ra0 = 1
.src_ref 0 "signal_path.c" 214 14 first
	/* 0x000010 0x84048 */    a0[0x0] = ra0
.src_ref 0 "signal_path.c" 216 14
	/* 0x000011 0xa0020 */    a0 = a0 + 0x4
	/* 0x000012 0x881e0 */    sp[0xc] = a0
.src_ref 0 "signal_path.c" 215 25 first
	/* 0x000013 0x66000 */    calldb _Z16int32_to_float64i
	/* 0x000014 0x00008 */    /* MW */
.src_ref 0 "signal_path.c" 215 25
	/* 0x000015 0x88088 */    ra0 = sp[0x4]
.src_ref 0 "signal_path.c" 215 20
	/* 0x000016 0x2a002 */    bx0 = ax0 + 0x0
.src_ref 0 "signal_path.c" 215 20
	/* 0x000017 0x66000 */    calldb ff_pow
	/* 0x000018 0x00008 */    /* MW */
.src_ref 0 "signal_path.c" 215 20
	/* 0x000019 0x6e000 */    axl1 = [(_ro_lbl_DM_8___Z10set_weightP16SingleSignalPathdi_8_1 + 0)]
	/* 0x00001a 0x00411 */    /* MW */
.src_ref 0 "signal_path.c" 215 40
	/* 0x00001b 0x2a001 */    ax1 = ax0 + 0x0
.src_ref 0 "signal_path.c" 215 40
	/* 0x00001c 0x66000 */    calldb _Z11float64_subyy
	/* 0x00001d 0x00008 */    /* MW */
.src_ref 0 "signal_path.c" 215 40
	/* 0x00001e 0x6e000 */    bxl0 = [_ro_lbl_DM_8___Z10set_weightP16SingleSignalPathdi_0_0]
	/* 0x00001f 0x00012 */    /* MW */
.src_ref 0 "signal_path.c" 215 40
	/* 0x000020 0x66000 */    call _Z30float64_to_int32_round_to_zeroy
	/* 0x000021 0x00000 */    /* MW */
.src_ref 0 "signal_path.c" 216 32 first
	/* 0x000022 0x66000 */    call _Z16int32_to_float64i
	/* 0x000023 0x00000 */    /* MW */
.src_ref 0 "signal_path.c" 216 32
	/* 0x000024 0x66000 */    calldb _Z11float64_mulyy
	/* 0x000025 0x00008 */    /* MW */
.src_ref 0 "signal_path.c" 216 32
.src_ref 0 "signal_path.c" 216 32
	/* 0x000026 0x55001 */    bx0 = ax0 + 0x0; axl1 = sp[0x10]
	/* 0x000027 0x10211 */    /* MW */
.src_ref 0 "signal_path.c" 216 23
	/* 0x000028 0x66000 */    call _Z30float64_to_int32_round_to_zeroy
	/* 0x000029 0x00000 */    /* MW */
.src_ref 0 "signal_path.c" 217 14
	/* 0x00002a 0x881a1 */    a1 = sp[0xc]
.src_ref 0 "signal_path.c" 216 14
	/* 0x00002b 0x88120 */    a0 = sp[0x8]
.src_ref 0 "signal_path.c" 217 14
	/* 0x00002c 0x8808a */    rb0 = sp[0x4]
.src_ref 0 "signal_path.c" 219
	/* 0x00002d 0x88036 */    lr = sp[0x0]
.src_ref 0 "signal_path.c" 216 14
	/* 0x00002e 0x42027 */    jpsdb 0x4; a0[0x4] = ra0
	/* 0x00002f 0x840c8 */    /* MW */
.src_ref 0 "signal_path.c" 217 14 first
	/* 0x000030 0x848ca */    a1[0x4] = rb0
.src_ref 0 "signal_path.c" 219
	/* 0x000031 0x88036 */    lr = sp[0x0]
.src_ref 0 "signal_path.c" 210 14 first
	/* 0x000032 0x40000 */    nop; a0[0x0] = zero
	/* 0x000033 0x0407a */    /* MW */
.label _Z10set_weightP16SingleSignalPathdi__end last
.src_ref 0 "signal_path.c" 219 first
.src_ref 0 "signal_path.c" 219 first
	/* 0x000034 0x460a0 */    ret; sp+= 0x18
	/* 0x000035 0x28030 */    /* MW */

.undef global text ff_pow

.undef global text _Z10float64_eqyy

.undef global text _Z16int32_to_float64i

.undef global text _Z11float64_subyy

.undef global text _Z30float64_to_int32_round_to_zeroy

.undef global text _Z11float64_mulyy

.data_segment_name
.rodata.constmem global 8 _ro_data_DM_8___Z17initialize_signalP16SingleSignalPathS0_PdS1_iidddi__1 DM
.label _ro_lbl_DM_8___Z17initialize_signalP16SingleSignalPathS0_PdS1_iidddi_0_0
	0x0
	0x0
	0xc0
	0xff
	0xff
	0xff
	0xdf
	0x41

.text_segment_name
.text global 2 _Z17initialize_signalP16SingleSignalPathS0_PdS1_iidddi
.src_ref 0 "signal_path.c" 296 first
.src_ref 0 "signal_path.c" 296 5
	/* 0x000000 0xabf80 */    sp+= -0x40
	/* 0x000001 0x90758 */    sp[0x38] = ahl0
	/* 0x000002 0x90659 */    sp[0x30] = ahl1
	/* 0x000003 0x9055a */    sp[0x28] = bhl0
	/* 0x000004 0x883f6 */    sp[0x1c] = lr
	/* 0x000005 0x88448 */    sp[0x20] = ra0
	/* 0x000006 0x8814a */    sp[0x8] = rb0
	/* 0x000007 0x881c9 */    sp[0xc] = ra1
	/* 0x000008 0x88263 */    sp[0x10] = a3
	/* 0x000009 0x882e1 */    sp[0x14] = a1
	/* 0x00000a 0x88360 */    sp[0x18] = a0
.src_ref 0 "signal_path.c" 311 47
.src_ref 0 "signal_path.c" 311 55
.src_ref 0 "signal_path.c" 311 63
	/* 0x00000b 0x39040 */    c0 = 8
.src_ref 0 "signal_path.c" 311 47 first
	/* 0x00000c 0x8d010 */    axl0 = [a2+c0]
.src_ref 0 "signal_path.c" 311 55
	/* 0x00000d 0x8d011 */    axl1 = [a2+c0]
.src_ref 0 "signal_path.c" 311 63
	/* 0x00000e 0x8d012 */    bxl0 = [a2+c0]
.src_ref 0 "signal_path.c" 311 79
	/* 0x00000f 0x8d133 */    bxl1 = a2[0x8]
	/* 0x000010 0x9005b */    sp[0x0] = bhl1
.src_ref 0 "signal_path.c" 311 4
	/* 0x000011 0x66000 */    calldb _Z20scale_preemph_filterP16SingleSignalPathdddddi
	/* 0x000012 0x00008 */    /* MW */
.src_ref 0 "signal_path.c" 311 4
.src_ref 0 "signal_path.c" 311 71
	/* 0x000013 0x5c07e */    ra0 = 31; bxl1 = a2[0x0]
	/* 0x000014 0x0d033 */    /* MW */
.src_ref 0 "signal_path.c" 312 4
	/* 0x000015 0x88320 */    a0 = sp[0x18]
.src_ref 0 "signal_path.c" 312 4 first
	/* 0x000016 0x66000 */    calldb _Z9set_delayP16SingleSignalPathi
	/* 0x000017 0x00008 */    /* MW */
.src_ref 0 "signal_path.c" 312 4
	/* 0x000018 0x88409 */    ra1 = sp[0x20]
.src_ref 0 "signal_path.c" 313 4
	/* 0x000019 0x88320 */    a0 = sp[0x18]
.src_ref 0 "signal_path.c" 313 4 first
	/* 0x00001a 0x66000 */    calldb _Z10set_weightP16SingleSignalPathdi
	/* 0x00001b 0x00008 */    /* MW */
.src_ref 0 "signal_path.c" 313 4
.src_ref 0 "signal_path.c" 313 4
	/* 0x00001c 0x5c07e */    ra0 = 31; axl0 = sp[0x38]
	/* 0x00001d 0x10710 */    /* MW */
.src_ref 0 "signal_path.c" 316 51
	/* 0x00001e 0x88222 */    a2 = sp[0x10]
.src_ref 0 "signal_path.c" 316 4
.src_ref 0 "signal_path.c" 316 51
.src_ref 0 "signal_path.c" 316 61
.src_ref 0 "signal_path.c" 316 71
	/* 0x00001f 0x5c820 */    c0 = 8; a0 = sp[0x14]
	/* 0x000020 0x082a0 */    /* MW */
.src_ref 0 "signal_path.c" 316 4
.src_ref 0 "signal_path.c" 316 51 first
	/* 0x000021 0x5c07e */    ra0 = 31; axl0 = [a2+c0]
	/* 0x000022 0x0d010 */    /* MW */
.src_ref 0 "signal_path.c" 316 61
	/* 0x000023 0x8d011 */    axl1 = [a2+c0]
.src_ref 0 "signal_path.c" 316 71
	/* 0x000024 0x8d012 */    bxl0 = [a2+c0]
.src_ref 0 "signal_path.c" 316 91
	/* 0x000025 0x8d133 */    bxl1 = a2[0x8]
	/* 0x000026 0x9005b */    sp[0x0] = bhl1
.src_ref 0 "signal_path.c" 316 4
	/* 0x000027 0x66000 */    calldb _Z20scale_preemph_filterP16SingleSignalPathdddddi
	/* 0x000028 0x00008 */    /* MW */
.src_ref 0 "signal_path.c" 316 81
	/* 0x000029 0x8d033 */    bxl1 = a2[0x0]
.src_ref 0 "signal_path.c" 317 4
	/* 0x00002a 0x882a0 */    a0 = sp[0x14]
.src_ref 0 "signal_path.c" 317 4 first
	/* 0x00002b 0x66000 */    calldb _Z9set_delayP16SingleSignalPathi
	/* 0x00002c 0x00008 */    /* MW */
.src_ref 0 "signal_path.c" 317 4
	/* 0x00002d 0x88189 */    ra1 = sp[0xc]
.src_ref 0 "signal_path.c" 318 4
	/* 0x00002e 0x882a0 */    a0 = sp[0x14]
.src_ref 0 "signal_path.c" 318 4 first
	/* 0x00002f 0x66000 */    calldb _Z10set_weightP16SingleSignalPathdi
	/* 0x000030 0x00008 */    /* MW */
.src_ref 0 "signal_path.c" 318 4
.src_ref 0 "signal_path.c" 318 4
	/* 0x000031 0x5c07e */    ra0 = 31; axl0 = sp[0x30]
	/* 0x000032 0x10610 */    /* MW */
.src_ref 0 "signal_path.c" 322 16
	/* 0x000033 0x90511 */    axl1 = sp[0x28]
.src_ref 0 "signal_path.c" 322 16 first
	/* 0x000034 0x66000 */    calldb _Z11float64_mulyy
	/* 0x000035 0x00008 */    /* MW */
.src_ref 0 "signal_path.c" 322 16
	/* 0x000036 0x6e000 */    bxl0 = [_ro_lbl_DM_8___Z17initialize_signalP16SingleSignalPathS0_PdS1_iidddi_0_0]
	/* 0x000037 0x00012 */    /* MW */
.src_ref 0 "signal_path.c" 322 7
	/* 0x000038 0x66000 */    call _Z30float64_to_int32_round_to_zeroy
	/* 0x000039 0x00000 */    /* MW */
.src_ref 0 "signal_path.c" 322 4
	/* 0x00003a 0x6c000 */    [_ZL2mu] = ra0
	/* 0x00003b 0x00048 */    /* MW */
.src_ref 0 "signal_path.c" 324 4
	/* 0x00003c 0x68000 */    a4 = pointer_sample_line
	/* 0x00003d 0x00024 */    /* MW */
.src_ref 0 "signal_path.c" 324 4
	/* 0x00003e 0x68000 */    a5 = sample_line
	/* 0x00003f 0x00025 */    /* MW */
.src_ref 0 "signal_path.c" 324 4 first
	/* 0x000040 0x66000 */    calldb _Z21initialize_buffer_dmbPU17chess_storage_DMB12BufferPtrDMBPU17chess_storage_DMBiii
	/* 0x000041 0x00008 */    /* MW */
.src_ref 0 "signal_path.c" 324 4
.src_ref 0 "signal_path.c" 324 4
	/* 0x000042 0x5c0b7 */    rb0 = 45; ra1 = sp[0x8]
	/* 0x000043 0x08109 */    /* MW */
.src_ref 0 "signal_path.c" 325 4
	/* 0x000044 0x68000 */    a0 = pointer_coefficient_line
	/* 0x000045 0x00020 */    /* MW */
.src_ref 0 "signal_path.c" 325 4
	/* 0x000046 0x68000 */    a1 = coefficient_line
	/* 0x000047 0x00021 */    /* MW */
.src_ref 0 "signal_path.c" 325 4 first
	/* 0x000048 0x66000 */    calldb _Z17initialize_bufferP9BufferPtrPiii
	/* 0x000049 0x00008 */    /* MW */
.src_ref 0 "signal_path.c" 325 4
.src_ref 0 "signal_path.c" 325 4
	/* 0x00004a 0x5c0b7 */    rb0 = 45; ra1 = sp[0x8]
	/* 0x00004b 0x08109 */    /* MW */
.src_ref 0 "signal_path.c" 328 4
	/* 0x00004c 0x88108 */    ra0 = sp[0x8]
.src_ref 0 "signal_path.c" 328 4 first
	/* 0x00004d 0x32020 */    cmp(ra0,0x0)
.src_ref 0 "signal_path.c" 328 4
	/* 0x00004e 0xbc0d5 */    if (np) jps 0xd
.src_ref 0 "signal_path.c" 329 27 first
	/* 0x00004f 0x6c000 */    a0 = [(pointer_sample_line + 4)]
	/* 0x000050 0x00220 */    /* MW */
.src_ref 0 "signal_path.c" 328 4 first
	/* 0x000051 0x62000 */    lp [ra0] 0x3
	/* 0x000052 0x00034 */    /* MW */
.src_ref 0 "signal_path.c" 330 32 first
	/* 0x000053 0x6c000 */    a2 = [(pointer_coefficient_line + 4)]
	/* 0x000054 0x00222 */    /* MW */
.src_ref 0 "signal_path.c" 329 37
.src_ref 0 "signal_path.c" 330 42
.src_ref 0 "signal_path.c" 332
	/* 0x000055 0x5c810 */    c0 = 4; lr = sp[0x1c]
	/* 0x000056 0x083b6 */    /* MW */
.src_ref 0 "signal_path.c" 329 37 first
	/* 0x000057 0x8007a */    [a0+c0] = zero
.src_ref 0 "signal_path.c" 330 42 first
	/* 0x000058 0x40000 */    nop; [a2+c0] = zero
	/* 0x000059 0x0107a */    /* MW */
.src_ref 0 "signal_path.c" 332 first
.src_ref 0 "signal_path.c" 332 first
	/* 0x00005a 0x460a0 */    ret; sp+= 0x40
	/* 0x00005b 0x28080 */    /* MW */
.label _Z17initialize_signalP16SingleSignalPathS0_PdS1_iidddi__end last
.src_ref 0 "signal_path.c" 332
	/* 0x00005c 0x43fe3 */    jps -0x4; lr = sp[0x1c]
	/* 0x00005d 0x883b6 */    /* MW */

.undef global data pointer_sample_line

.undef global data sample_line

.undef global data pointer_coefficient_line

.undef global data coefficient_line

.undef global text _Z20scale_preemph_filterP16SingleSignalPathdddddi

.undef global text _Z9set_delayP16SingleSignalPathi

.undef global text _Z10set_weightP16SingleSignalPathdi

.undef global text _Z21initialize_buffer_dmbPU17chess_storage_DMB12BufferPtrDMBPU17chess_storage_DMBiii

.undef global text _Z17initialize_bufferP9BufferPtrPiii

.undef global text _Z11float64_mulyy

.undef global text _Z30float64_to_int32_round_to_zeroy

.text_segment_name
.text global 2 _Z16calculate_outputP4FILEP16SingleSignalPathS2_PU17chess_storage_DMBVsS4_S4_
.src_ref 0 "signal_path.c" 336 first
.src_ref 0 "signal_path.c" 361 47 first
	/* 0x000000 0x96034 */    ra0.s = a4[0x0]
.src_ref 0 "signal_path.c" 361 52 first
.src_ref 0 "signal_path.c" 362 50 first
	/* 0x000001 0x51a13 */    rb0 = lsl(ra0,0x10); ra0.s = a5[0x0]
	/* 0x000002 0x16834 */    /* MW */
.src_ref 0 "signal_path.c" 336 5
.src_ref 0 "signal_path.c" 362 55
	/* 0x000003 0x51a12 */    ra0 = lsl(ra0,0x10); sp+= -0x8
	/* 0x000004 0x2bff0 */    /* MW */
	/* 0x000005 0x88076 */    sp[0x0] = lr
.src_ref 0 "signal_path.c" 373 4
	/* 0x000006 0x68000 */    a4 = pointer_sample_line
	/* 0x000007 0x00024 */    /* MW */
.src_ref 0 "signal_path.c" 361 19
	/* 0x000008 0x6c000 */    [_ZZ16calculate_outputP4FILEP16SingleSignalPathS2_PU17chess_storage_DMBVsS4_S4_E11c_sensor_32] = rb0
	/* 0x000009 0x0004a */    /* MW */
.src_ref 0 "signal_path.c" 366 21 first
	/* 0x00000a 0x6c000 */    [_ZZ16calculate_outputP4FILEP16SingleSignalPathS2_PU17chess_storage_DMBVsS4_S4_E12c_sensor_pre] = rb0
	/* 0x00000b 0x0004a */    /* MW */
.src_ref 0 "signal_path.c" 362 21 first
	/* 0x00000c 0x6c000 */    [_ZZ16calculate_outputP4FILEP16SingleSignalPathS2_PU17chess_storage_DMBVsS4_S4_E13acc_sensor_32] = ra0
	/* 0x00000d 0x00048 */    /* MW */
.src_ref 0 "signal_path.c" 367 23 first
	/* 0x00000e 0x6c000 */    [_ZZ16calculate_outputP4FILEP16SingleSignalPathS2_PU17chess_storage_DMBVsS4_S4_E14acc_sensor_pre] = ra0
	/* 0x00000f 0x00048 */    /* MW */
.src_ref 0 "signal_path.c" 373 4 first
	/* 0x000010 0x66000 */    call _Z16write_buffer_dmbPU17chess_storage_DMB12BufferPtrDMBi
	/* 0x000011 0x00000 */    /* MW */
.src_ref 0 "signal_path.c" 376 28
	/* 0x000012 0x68000 */    a4 = pointer_sample_line
	/* 0x000013 0x00024 */    /* MW */
.src_ref 0 "signal_path.c" 376 28
.src_ref 0 "signal_path.c" 380 4
	/* 0x000014 0x68000 */    a2 = pointer_coefficient_line
	/* 0x000015 0x00022 */    /* MW */
.src_ref 0 "signal_path.c" 376 28 first
	/* 0x000016 0x6c000 */    a0 = [(pointer_coefficient_line + 8)]
	/* 0x000017 0x00420 */    /* MW */
.src_ref 0 "signal_path.c" 376 28
.src_ref 0 "signal_path.c" 376 28
	/* 0x000018 0x5c810 */    c0 = 4; a4 = a4 + 0x8
	/* 0x000019 0x22044 */    /* MW */
.src_ref 0 "signal_path.c" 376 28
	/* 0x00001a 0x82225 */    a5 = [a4-c0]
.src_ref 0 "signal_path.c" 376 28
	/* 0x00001b 0x8222c */    lb0 = [a4-c0]
.src_ref 0 "signal_path.c" 376 28
	/* 0x00001c 0x40000 */    nop; ra0 = a4[0x0]
	/* 0x00001d 0x06008 */    /* MW */
.src_ref 0 "signal_path.c" 376 28
.src_ref 0 "signal_path.c" 376 28
	/* 0x00001e 0x51852 */    ra0 = lsl(ra0,0x2); rb0 = a2[0x0]
	/* 0x00001f 0x0500a */    /* MW */
.src_ref 0 "signal_path.c" 376 28
.src_ref 0 "signal_path.c" 380 4
	/* 0x000020 0x553fa */    ra0 = rb0 + -0x1; lsz0 = ra0
	/* 0x000021 0x1822e */    /* MW */
.src_ref 0 "signal_path.c" 376 28
.src_ref 0 "signal_path.c" 380 4
	/* 0x000022 0x51432 */    ra0 = asr(ra0,0x1); c1 = -0x4
	/* 0x000023 0x2ffe1 */    /* MW */
.src_ref 0 "signal_path.c" 384 19
.src_ref 0 "signal_path.c" 384 23
	/* 0x000024 0x55033 */    rb1 = ra0 + 0x1; a1 = sp[0x8]
	/* 0x000025 0x88121 */    /* MW */
.src_ref 0 "signal_path.c" 376 28
	/* 0x000026 0x62000 */    lp [rb1] 0x4
	/* 0x000027 0x00047 */    /* MW */
.src_ref 0 "signal_path.c" 376 28
.src_ref 0 "signal_path.c" 376 28
	/* 0x000028 0x5c001 */    bx0 = 0; a4 = a5 + 0x0
	/* 0x000029 0x22804 */    /* MW */
.src_ref 0 "signal_path.c" 376 28
.src_ref 0 "signal_path.c" 376 28
.src_ref 0 "signal_path.c" 376 28
.src_ref 0 "signal_path.c" 376 28
	/* 0x00002a 0x5c000 */    ax0 = 0; ra1 = [a0+c0]; rb0 = [a4+%0c1]
	/* 0x00002b 0x58089 */    /* MW */
.src_ref 0 "signal_path.c" 376 28
.src_ref 0 "signal_path.c" 376 28
.src_ref 0 "signal_path.c" 376 28
.src_ref 0 "signal_path.c" 376 28
	/* 0x00002c 0x444d4 */    bx0 = bx0+rb0*ra1; ra0 = [a0+c0]; rb0 = [a4+%0c1]
	/* 0x00002d 0x50089 */    /* MW */
.src_ref 0 "signal_path.c" 376 28
.src_ref 0 "signal_path.c" 376 28
.src_ref 0 "signal_path.c" 376 28
.src_ref 0 "signal_path.c" 376 28
	/* 0x00002e 0x44440 */    ax0 = ax0+rb0*ra0; ra1 = [a0+c0]; rb0 = [a4+%0c1]
	/* 0x00002f 0x58089 */    /* MW */
.src_ref 0 "signal_path.c" 378 31 first
	/* 0x000030 0x6c000 */    rb0 = [_ZZ16calculate_outputP4FILEP16SingleSignalPathS2_PU17chess_storage_DMBVsS4_S4_E12c_sensor_pre]
	/* 0x000031 0x0000a */    /* MW */
.src_ref 0 "signal_path.c" 376 28 first
.src_ref 0 "signal_path.c" 380 4 first
	/* 0x000032 0x54008 */    ax0 = bx0 + ax0; a4 = a2[0x4]
	/* 0x000033 0x050a4 */    /* MW */
.src_ref 0 "signal_path.c" 376 28
.src_ref 0 "signal_path.c" 380 4
	/* 0x000034 0x5cbe0 */    c0 = -8; ra0 = axs0
	/* 0x000035 0x18008 */    /* MW */
.src_ref 0 "signal_path.c" 376 22
	/* 0x000036 0x6c000 */    [_ZZ16calculate_outputP4FILEP16SingleSignalPathS2_PU17chess_storage_DMBVsS4_S4_E18filter_accumulator] = ra0
	/* 0x000037 0x00048 */    /* MW */
.src_ref 0 "signal_path.c" 378 35 first
.src_ref 0 "signal_path.c" 380 4 first
	/* 0x000038 0x5709a */    ra0 = rb0 - ra0; a0 = a5+%0c1
	/* 0x000039 0x1ec80 */    /* MW */
.src_ref 0 "signal_path.c" 380 4
	/* 0x00003a 0x6c000 */    rb0 = [_ZL2mu]
	/* 0x00003b 0x0000a */    /* MW */
.src_ref 0 "signal_path.c" 380 4
.src_ref 0 "signal_path.c" 380 4
	/* 0x00003c 0x44400 */    ax0 = rb0*ra0; c1 = 0x8
	/* 0x00003d 0x2c041 */    /* MW */
.src_ref 0 "signal_path.c" 380 4
	/* 0x00003e 0x62000 */    lp [rb1] 0x7
	/* 0x00003f 0x00077 */    /* MW */
.src_ref 0 "signal_path.c" 378 13
	/* 0x000040 0x6c000 */    [_ZZ16calculate_outputP4FILEP16SingleSignalPathS2_PU17chess_storage_DMBVsS4_S4_E9output_32] = ra0
	/* 0x000041 0x00048 */    /* MW */
.src_ref 0 "signal_path.c" 380 4
	/* 0x000042 0x98009 */    ra1 = axs0
.src_ref 0 "signal_path.c" 380 4
	/* 0x000043 0x8e025 */    axs1,bxs1 = a4[0x0]
.src_ref 0 "signal_path.c" 380 4
.src_ref 0 "signal_path.c" 380 4
	/* 0x000044 0x82c08 */    ra0 = [a5+%0c0]
.src_ref 0 "signal_path.c" 380 4
.src_ref 0 "signal_path.c" 380 4
.src_ref 0 "signal_path.c" 380 4
	/* 0x000045 0x44242 */    ax0 = ax1+ra1*ra0; rb0 = [a0+%0c0]
	/* 0x000046 0x0040a */    /* MW */
.src_ref 0 "signal_path.c" 380 4
	/* 0x000047 0x086ac */    bx0 = bx1+ra1*rb0
.src_ref 0 "signal_path.c" 380 4
	/* 0x000048 0x8e0c0 */    [a4+c1] = axs0,bxs0
	/* 0x000049 0x00000 */    nop
.src_ref 0 "signal_path.c" 384 56 first
	/* 0x00004a 0x6c000 */    ra0 = [_ZZ16calculate_outputP4FILEP16SingleSignalPathS2_PU17chess_storage_DMBVsS4_S4_E9output_32]
	/* 0x00004b 0x00008 */    /* MW */
.src_ref 0 "signal_path.c" 384 61
.src_ref 0 "signal_path.c" 387
	/* 0x00004c 0x51610 */    ax0 = asr(ra0,0x10); lr = sp[0x0]
	/* 0x00004d 0x08036 */    /* MW */
.src_ref 0 "signal_path.c" 384 25
.src_ref 0 "signal_path.c" 387 first
	/* 0x00004e 0x460a4 */    retdb; axs0 = axs0
	/* 0x00004f 0x18000 */    /* MW */
.src_ref 0 "signal_path.c" 384 19 first
.src_ref 0 "signal_path.c" 384 23 first
	/* 0x000050 0x94870 */    a1[0x0] = axs0.s
.label _Z16calculate_outputP4FILEP16SingleSignalPathS2_PU17chess_storage_DMBVsS4_S4___end
.src_ref 0 "signal_path.c" 387 first
	/* 0x000051 0xa8010 */    sp+= 0x8

.undef global data pointer_sample_line

.undef global data pointer_coefficient_line

.undef global text _Z16write_buffer_dmbPU17chess_storage_DMB12BufferPtrDMBi

.dir 0 "C:/Users/phangl/00_Repos/06_DSP_Simulation/simulation/signal_processing"


.direct_eval +,-,(,)
